**Please see below link to how to start Yaskawa robotics arm**

1. **Turn on main switch**
2. **Check the emergency switch is released**
3. **Plug in the key**
4. **Move the black switch on position**

**https://youtu.be/mVhWDYZJv4I**